* **Power supply: AC100V-240V 50-60Hz**
* • **Maximum power: 1800W**
* • **Light source: 37 40W four in one LED**
* **beads**
* • **Color temperature: 2800K-8500K LED**
* **lifespan: 50000 hours**
* • **Display: Color screen flicker: 1-25**
* **times/second**
* • **Spot angle: 5.5-55 °**
* • **Dimming: 0-100% linear electronic**
* **dimming**
* • **Control mode: DMX512, RDM, self-**
* **propelled, or (ArtNet, sACN, and KingNet**
* **functions) optional**
* • **Channel mode: 22/36/111/148CH**
* • **Functional effects: Equipped with a color**
* **mixing correction system, CTO, staining,**
* **and beam,**
* • **Effect modes (Vortex, Kaleidoscope)**
* • **The front mirror disc can rotate infinitely**
* **and seamlessly connect mirror discs,**
* •
* **Non spherical lens structure, single point**
* **control of lamp bead**
* •
* **size:72\*40\*62cm carton weight: 28kg**