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25-channel mode
	channel
	function
	explain

	CH1
	Central dimming
	Central dimming, from dim to bright

	CH2
	RGBW strobe lighting
	RGBW strobe lighting, from slow to fast

	CH3
	R dimming
	R dimming, from dim to bright

	CH4
	G dimming
	G dimming, from dim to bright

	CH5
	B dimming
	B dimming, from dim to bright

	CH6
	Dimming
	Dimming, from dim to bright

	CH7
	RGBW running code
	0-65 RGBW running effects

	CH8
	RGBW scanning speed
	RGBW running speed, from slow to fast: 0–128 forward, 129–255 backward

	CH9
	R background colour
	R background tone light, from dim to light

	CH10
	G background colour
	G background tone light, from dim to light

	CH11
	B background colour
	B Background tone light, from dim to bright

	CH12
	W background colour
	Background tone light, from dim to bright

	CH13
	R1, G1, B1 strobe
	R1, G1, B1 strobe light, from slow to fast

	CH14
	R1 dimming
	R1 dimming, from dim to bright

	CH15
	G1 dimming
	G1 dimming, from dim to bright

	CH16
	B1 dimming
	B1 dimming, from dim to bright

	CH17
	R1G1B1 run code
	0-65 types of R1G1B1 running effects

	CH18
	R1G1B1 code running speed
	The R1G1B1 running speed ranges from slow to fast: 0–128 forward, 129–255 reverse.

	CH19
	R1 background color
	R1 background tone light, from dim to bright

	CH20
	G1 background color
	G1 background tone light, from dim to bright

	CH21
	B1 background color
	B1 background tone light, from dim to bright

	CH22
	W1 dimming
	W1 dimming, from dim to bright

	CH23
	W1 Stroboscopic Light
	W1 strobe, from slow to fast

	CH24
	W1 Run Code
	0–30 W1 running effects

	CH25
	W1 running speed
	W1 running speed, from slow to fast: 0–128 forward, 129–255 backward


LED Par                          
24V power supply with a 12V auxiliary light
direction for use
=====Professional Stage Lighting Equipment========
230-channel mode
	channel
	function
	explain

	CH1
	5050-R1 dimming
	5050-R1 dimming, from dim to bright

	CH2
	5050-G1 dimming
	5050-G1 dimming, from dim to bright

	CH3
	5050-B1 dimming
	5050-B1 dimming, from dim to bright

	CH4
	5050-W1 dimming
	5050-W1 dimming, from dim to bright

	...
	...
	...

	CH20
	5050-R6 dimming
	5050-R6 dimming, from dim to bright

	CH21
	5050-G6 dimming
	5050-G6 dimming, from dim to bright

	CH22
	5050-B6 dimming
	5050-B6 dimming, from dim to bright

	CH23
	5050-W6 dimming
	5050-W6 dimming, from dim to bright

	CH24
	3030-R1 dimming
	3030-R1 dimming, from dim to bright

	CH25
	3030-G1 Dimming
	3030-G1 dimming, from dim to bright

	CH26
	3030-B1 dimming
	3030-B1 dimming, from dim to bright

	...
	...
	...

	CH129
	3030-R36 dimming
	3030-R36 dimming, from dim to bright

	CH130
	3030-G36 Dimming
	3030-G36 dimming, from dim to bright

	CH131
	3030-B36 Dimming
	3030-B36 dimming, from dim to bright

	CH132
	3030-W1-1 Dimming
	3030-W1-1 dimming, from dim to bright

	CH133
	3030-W1-2 Dimming
	3030-W1-2 dimming, from dim to bright

	CH134
	3030-W1-3 Dimming
	3030-W1-3 dimming, from dim to bright

	...
	...
	...

	CH180
	3030-W17-1 Dimming
	3030-W17-1 dimming, from dim to bright

	CH181
	3030-W17-2 Dimming
	3030-W17-2 dimming, from dim to bright

	CH182
	3030-W17-3 Dimming
	3030-W17-3 dimming, from dim to bright


8-channel mode
	channel
	function
	explain

	CH1
	R dimming
	R dimming, from dim to bright

	CH2
	G dimming
	G dimming, from dim to bright

	CH3
	B dimming
	B dimming, from dim to bright

	CH4
	Dimming
	Dimming, from dim to bright

	CH5
	R1 dimming
	R1 dimming, from dim to bright

	CH6
	G1 dimming
	G1 dimming, from dim to bright

	CH7
	B1 dimming
	B1 dimming, from dim to bright

	CH8
	W1 dimming
	W1 dimming, from dim to bright
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Input power: AC 90–240 V, wide voltage range input
Light source: WY 102 units, RGB 216 units, RGBW 18 units
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Channel configuration: 182/25/8 DMX512 control channels are configurable
Power consumption: Approximately 200W in total
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1. Button illustration:
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MENU: Function keys   UP: Increase key   DOWN: Decrease key   ENTER: Confirm key
MENU: Function keys   UP: Increase key DOWN: Decrease key   ENTER: Confirm key
MENU function key ：
Pressing the MENU function key cycles through the functions listed in Table (1). The first 1–2 digits on the digital display indicate the current function, while the subsequent 2–3 digits specify parameters such as speed and effects. Adjust these parameters by pressing the UP or DOWN key, then confirm with the ENTER key.
ENTER confirmation key:
Press this key to save the currently set parameter settings, which will be executed upon startup.
	UP key: Press this key to increase; hold for more than 2 seconds to increase continuously. DOWN key: Press this key to decrease; hold for more than 2 seconds to decrease continuously. Serial number
	content
	scale
	Function and Description

	1
	A001
	001- 512
	DMX512 channel address code setting

	2
	CH27
	8/25/230
	Channel Number Selection

	3
	FH99
	01-99
	Flicker, from slow to fast

	4
	CL01
	01-08
	8 commonly used color outputs.

	5
	LL99
	01 - 99
	A colorful transition, from slow to fast.

	6
	DE99
	01 - 99
	A seven-color gradient, transitioning from slow to fast.

	7
	CP99
	01 - 99
	The seven-colored pulse changes, progressing from slow to fast.

	8
	Su99
	01 - 99
	Voice sensitivity selection.

	9
	n060
	01-60
	The main light RGBW features 60 selectable effects.

	10
	S255
	1-255
	The RGBW primary light runs from slow to fast.

	11
	F066
	01-66
	The ambient light RGB mode offers 66 different effect options.

	12
	S255
	1-255
	The RGB1 fill light accelerates from slow to fast.

	13
	g032
	1-32
	The W Light Source offers 32 different effect options for running scenes.

	14
	S255
	1-255
	The fill light W accelerates from slow to fast.

	15
	r255
	000- 255
	Red dimming, from dim to bright.

	16
	g255
	000- 255
	G: Green dimming, from dim to bright.

	17
	b255
	000- 255
	B Blue dimming, from dim to bright.

	18
	u255
	000- 255
	White dimming, from dim to bright.

	19
	r255
	000- 255
	R1 red dimming, from dim to bright.

	20
	g255
	000- 255
	G1 green dimming, from dim to bright.

	21
	b255
	000- 255
	B1 blue dimming, from dim to bright.

	22
	u255
	000- 255
	W1 white dimming, from dim to bright.

	order
	content
	scale
	Function and Description

	1
	0601
	-
	version number

	2
	R160
	0-255
	R Current Regulation

	3
	G160
	0-255
	G Current Regulation

	4
	B160
	0-255
	B Current Regulation

	5
	W160
	0-255
	Current Regulation

	6
	1160
	0-255
	R1 current regulation

	7
	2160
	0-255
	G1 current regulation

	8
	3160
	0-255
	B1 current regulation

	9
	4160
	0-255
	W1 Current Regulation

	10
	rgbu
	-
	Full Light

	11
	cr04
	-
	Color Mode Selection

	12
	PG00
	00--66
	Click-to-activate current

	13
	tL55
	50-80
	Power Protection

	14
	p222
	50-250
	Current Adjustment

	15
	tg01
	1-30
	Dimming level

	16
	CH02
	-
	Channel Mode Selection

	17
	bc01
	0-3
	512 Signal Holding Setting

	18
	Ft40
	35-70
	Temperature Protection

	19
	pb00
	00-05
	screensaver selection


Table (II) Comparison Table of Backend Functions
Table (I) Comparison Table of Digital Display Window Functions
DMX Channel Description





Performance Features and Technical Specifications








Button Operation Instructions








